Annex. 1. Technical specification for the supply of the following items:

LOT № 1. TV

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | LED Smart TV | Size: 43 "(109 cm)  Display Type: IPS  Aspect Ratio: 16: 9  Screen Viewing Angle: 178 °  CPU Cores: 1  TV tuner: DVB-T ½, C, S  Network: LAN, Wi-Fi (gbn), BT  Connectivity: 2 x HDMI 1.4 (ARC; CEC), satellite input (main; F-type jack), antenna (RF), USB, Ethernet RJ45  Built-in media player: (photo, audio, video)  Audio speakers: 2 x 5 W  OS: Smart TV  Wall Mount - VESA Mount: Yes  220-240 V, 50 - 60 Hz  Energy Class: A +  remote control | pcs | 15 | Ministry of Education of the Republic of Tajikistan  Address: N.Muhammad St. 13, Dushanbe |
|  |  |  |  |  |  |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 2 | LED Smart TV | Size: 32 "(81 cm)  Display Type: IPS  Aspect Ratio: 16: 9  Screen Viewing Angle: 178 °  CPU Cores: 1  TV tuner: DVB-T ½, C, S  Network: LAN, Wi-Fi (gbn), BT  Connectivity: 2 x HDMI 1.4 (ARC; CEC), satellite input (main; F-type jack), antenna (RF), USB, Ethernet RJ45  Built-in media player: (photo, audio, video)  Audio speakers: 2 x 5 W  OS: Smart TV  Wall Mount - VESA Mount: Yes  220-240 V, 50 - 60 Hz  Energy Class: A +  remote control | pcs | 10 | delivery and installation of (equipment) to the support victim rooms in medical facilities of the following cities and areas    DRS: Dushanbe, Rudaki and Gissar.  Khatlon region: Yavan Vose and A.Jomi  Soghd region: B. Ghafurov, Isfara, Istaravshan, Aini, Penjikent. |

LOT № 2. Videoconferencing system

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | Videoconferencing system | Video conference system set: Camera PTZ FullHD 1080p; 12x zoom; movement step 0,45° x 0,25° (remote control), USB;  Speaker 10 W, 95 dB; Microphones: 2-3 built in 360° up to 6m; echo off; noise cancelation | pc. | 5 | four pcs. to Statistics Agency of the Republic of Tajikistan  Address: pr. Rudaki No. 40, Dushanbe  One pc. to Institute of Economy & Demography, Address: Ayni St. No. 44, Dushanbe |

LOT № 3. Projector screen/interactive board and projector

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | Interactive board | Full set: SMART Interactive Board min 77", + original software, ultra-short focus projector, DLP, Full HD 1080, 3500 Lm, 10000:1, 3D(optional), original wall mount system | Set | 1 | Institute of Economy & Demography, Address: Ayni St. No. 44, Dushanbe |
| 2 | Projector |
| 3 | Projector screen |

LOT № 4. Air Conditioner

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | Air conditioner: (split system) | Type of air conditioner: Split system  Service Area - 40 m2  Energy class: А (Inverter)  Maximum length of communications: 20 m  Basic modes: cooling/heating;  Additional modes: ventilation mode, automatic temperature maintenance, self-diagnosis;  Other functions: adjust air flow, anti-ice system;  Minimum temperature for operating the air conditioner in heating/cooling mode: -15 ° С  Power consumption for heating: 1520 W;  Power consumption for cooling: 1560 W;  Remote control: yes;  Adjustment of fan rotation speed: yes;  Number of speeds - min 3;  Refrigerant type: R 410A;  Phase: single phase | pcs. | 10 | delivery and installation of (equipment) to the support victim rooms in medical facilities of the following cities and areas    DRS: Dushanbe, Rudaki and Gissar.  Khatlon region: Yavan Vose and A.Jomi  Soghd region: B. Ghafurov, Isfara, Istaravshan, Aini, Penjikent. |

LOT № 4 Air Conditioner

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 2 | Air conditioner - columned | Type of air conditioner - columned  Service Area - 50 m2  The maximum length of communications - 20 m  Energy class - A  Basic functions - cooling / heating  Additional functions - ventilation mode (without cooling and heating), automatic temperature maintenance, self-diagnosis of malfunctions, drain mode  Remote control, Display  Type of refrigerant - R 410A  Phase - single phase  Fan speed adjustment  Other functions and features - the ability to adjust the airflow direction, anti-ice system, memory settings, display  The minimum temperature for operating the air conditioner in heating mode - -7 ° C  Additional heater for heating with a power of 2500 W (optional) | pcs. | 1 | Institute of Economy & Demography,  Address: Ayni St. No. 44, Dushanbe |

LOT № 5. Laptop with Docking Station

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | Laptop | Laptop: CPU Intel Core i7 9-10th gen min 2.20 GHz /RAM - 16GB memory/HDD 512 SSD / 13-14" Led screen/ Built-in 1000 Mbps Ethernet (RJ-45) /Wireless-B+G+N+AC +4G Modem(optional)/ Built-in HD webcam /3 x USB 3.0/ 8-in-1 media reader / min 4-6 cell battery pack, + docking station, + carrying case | pcs. | 2 | UNFPA Office  Address: Aini Street No. 48,  BC "Cозидание"  7th floor, block A  Dushanbe |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **№** | **Item** | **Technical specifications** | **Unit** | **Q-ty** | **Delivery & Installation Recipient** |
| 1 | Docking station | Docking station: Docking Interface USB-C, Video Interfaces: HDMI, 2 x DP, USB-C, Networking: Gigabit Ethernet, Power: Power adapter 180 Watt, Combo audio jack 3.5mm, Manufacturer Warranty: 3-year warranty. | pcs. | 2 | UNFPA Office  Address: Aini Street No. 48,  BC "Cозидание"  7th floor, block A  Dushanbe |
| 2 | Моnitor | Monitor: 27" LCD, IPS, Wide, 2k (2560x1440) or 4k (3840x2160), HDMI, DP, adjustment on height, USB3.0 Hub (optional). | Pcs. | 2 |
| 3 | Keyboard and mouse | Keyboard and mouse: Wireless Combo set, Performance keyboard, +laser wireless mouse, 3btn, Roll, FM, USB. | Pcs. | 2 |